Login authentication

Password:
<huawei>
Nov 30 2024 12:53:25+00:00 huawei LINE/4/USERLOGIN:OID 1.3.6.1.4.1.2011.5.25.207.2.2 A user login. (UserIndex=0, UserName=Console, UserIP=Console0, UserChannel=CON0)
<huawei>sys
Enter system view, return user view with Ctrl+Z.
[huawei]sysname LSW1
[LSW1]disp ip inter
[LSW1]disp ip interface br
[LSW1]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 4
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 5

Interface                         IP Address/Mask      Physical   Protocol
GigabitEthernet0/0/8              unassigned           down       down
GigabitEthernet0/0/9              unassigned           down       down
GigabitEthernet0/0/10             unassigned           up         down
NULL0                             unassigned           up         up(s)
Vlanif1                           192.168.1.1/24       down       down
XGigabitEthernet0/0/0             unassigned           down       down

[LSW1]sysname Huawei
[Huawei]q
<Huawei>q

  Info:Configuration console exit, please retry to log on

Login authentication

Username:
#Easy-Operation: Stop upgrading because of the input in the console.
#Easy-Operation: Enter the status of running normally.
Username:admin
Password:
Error: Authentication fail

Username:admin
Password:
Warning: The default password poses security risks.
The password needs to be changed. Change now? [Y/N]: y
Please enter old password:
Please enter new password:
Please confirm new password:
The password has been changed successfully.
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 12:47:52  Failed: 1

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<HUAWEI>sys
Enter system view, return user view with Ctrl+Z.
[HUAWEI]sysname LSW1
[LSW1]disp ip int
[LSW1]disp ip interface
Nov 30 2024 12:53:19 LSW1 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.3.1 configurations have been changed. The current change number is 130, the change loop count is 0, and the maximum number of records is 4095.
[LSW1]disp ip interface br
[LSW1]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 1
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 2

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down

[LSW1]
[LSW1]disp po
[LSW1]disp por
[LSW1]disp port
[LSW1]disp port i
[LSW1]disp port int
[LSW1]disp port
                ^
Error:Incomplete command found at '^' position.
[LSW1]disp port
[LSW1]disp portal
  Portal max-user number:640
  Quiet function is Enabled
  Different-server is Disabled
  Parameter set:Quiet Period        60s   Quiet-times         10
  Logout packets resend: Resend-times 3  Timeout 5s
  Portal Https Redirect: Enable
  Portal JS Redirect: Disable
  Portal 302 Redirect: Disable
[LSW1]disp port int
[LSW1]disp port int
                ^
Error: Unrecognized command found at '^' position.
[LSW1]disp ip inter
[LSW1]disp ip interface brie
[LSW1]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 1
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 2

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down

[LSW1]disp th
#
sysname LSW1
#
undo icmp name timestamp-request receive
#
ssh server cipher aes256_ctr aes128_ctr
ssh server hmac sha2_256
ssh client cipher aes256_ctr aes128_ctr
ssh client hmac sha2_256
ssh server dh-exchange min-len 2048
#
return
[LSW1]
Nov 30 2024 13:04:34 LSW1 %%01IFADP/4/PORTUPINFO(l)[0]:Interface GigabitEthernet0/0/4 has turned into UP state. (Information=Physical state: up, Negotiation: enable, Negotiation complete: yes, Local full-duplex(10M: yes, 100M: yes, 1000M: yes), Local half-duplex(10M: yes, 100M: yes, 1000M: no), Remote full-duplex(10M: yes, 100M: yes, 1000M: yes), Remote half-duplex(10M: yes, 100M: yes, 1000M: no))
[LSW1]
Nov 30 2024 13:04:36 LSW1 %%01IFPDT/4/IF_STATE(l)[1]:Interface GigabitEthernet0/0/4 has turned into UP state.
Nov 30 2024 13:04:36 LSW1 %%01MSTP/4/SET_PORT_DISCARDING(l)[2]:In MSTP process 0 instance 0, MSTP set port GigabitEthernet0/0/4 state as discarding.
[LSW1]
Nov 30 2024 13:04:36 LSW1 LLDP/4/NBRCHGTRAP:OID 1.0.8802.1.1.2.0.0.1 Neighbor information is changed. (LldpStatsRemTablesInserts=1, LldpStatsRemTablesDeletes=0, LldpStatsRemTablesDrops=0, LldpStatsRemTablesAgeouts=0)
[LSW1]interf
[LSW1]un in en
Info: Information center is disabled.
[LSW1]inte
[LSW1]interface eth-tru
[LSW1]interface Eth-Trunk 1
[LSW1-Eth-Trunk1]mode lacp
[LSW1-Eth-Trunk1]q
[LSW1]interf
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]eth-
[LSW1-GigabitEthernet0/0/3]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW1-GigabitEthernet0/0/3]int g0/0/5
[LSW1-GigabitEthernet0/0/5]int g0/0/4
[LSW1-GigabitEthernet0/0/4]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW1-GigabitEthernet0/0/4]q
[LSW1]lacp priority 100
[LSW1]in
[LSW1]int e
[LSW1]int Eth-Trunk 1
[LSW1-Eth-Trunk1]max active
[LSW1-Eth-Trunk1]max active-linknumber 2
[LSW1-Eth-Trunk1]q
[LSW1-Eth-Trunk1]q
[LSW1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]lacp pr
[LSW1-GigabitEthernet0/0/3]lacp priority 100
[LSW1-GigabitEthernet0/0/3]int g0/0/4
[LSW1-GigabitEthernet0/0/4]lacp priority 100
[LSW1-GigabitEthernet0/0/4]q
[LSW1]vlan ba
[LSW1]vlan batch 10 20
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]port
[LSW1-GigabitEthernet0/0/1]port lin
[LSW1-GigabitEthernet0/0/1]port link-t
[LSW1-GigabitEthernet0/0/1]port link-type ac
[LSW1-GigabitEthernet0/0/1]port link-type access
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW1-GigabitEthernet0/0/1]port de
[LSW1-GigabitEthernet0/0/1]port default vlan 10
[LSW1-GigabitEthernet0/0/1]q
[LSW1]int g0/0/2
[LSW1-GigabitEthernet0/0/2]port link-type ac
[LSW1-GigabitEthernet0/0/2]port link-type access
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW1-GigabitEthernet0/0/2]port de
[LSW1-GigabitEthernet0/0/2]port default vlan
[LSW1-GigabitEthernet0/0/2]port default vlan 30
[LSW1-GigabitEthernet0/0/2]port default vlan 20
[LSW1-GigabitEthernet0/0/2]q
[LSW1]
[LSW1]
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]q
[LSW1]int g0/0/5
[LSW1-GigabitEthernet0/0/5]eth-tr
[LSW1-GigabitEthernet0/0/5]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW1-GigabitEthernet0/0/5]q
[LSW1]int g/0/0/3
          ^
Error: Wrong parameter found at '^' position.
[LSW1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]port trunk allow-pass vlan 10 20
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]port link-type t
[LSW1-GigabitEthernet0/0/3]port link-type tr
[LSW1-GigabitEthernet0/0/3]port link-type trunk
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]disp this
#
interface GigabitEthernet0/0/3
 eth-trunk 1
 lacp priority 100
#
return
[LSW1-GigabitEthernet0/0/3]port lik
[LSW1-GigabitEthernet0/0/3]port lin
[LSW1-GigabitEthernet0/0/3]port link-t
[LSW1-GigabitEthernet0/0/3]port link-type trunk
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]undo portsw
[LSW1-GigabitEthernet0/0/3]int g0/0/1
[LSW1-GigabitEthernet0/0/1]disp this
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
#
return
[LSW1-GigabitEthernet0/0/1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]port link-
[LSW1-GigabitEthernet0/0/3]port link-t
[LSW1-GigabitEthernet0/0/3]port link-
[LSW1-GigabitEthernet0/0/3]port link-flap tru
[LSW1-GigabitEthernet0/0/3]port link-fla
[LSW1-GigabitEthernet0/0/3]port link-flap
                                          ^
Error:Incomplete command found at '^' position.
[LSW1-GigabitEthernet0/0/3]port link-flap 1
                                          ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]int g0/0/1
[LSW1-GigabitEthernet0/0/1]port link-t
[LSW1-GigabitEthernet0/0/1]port link-type trunk
Warning: This command will delete VLANs on this port. Continue?[Y/N]:n
[LSW1-GigabitEthernet0/0/1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]port link-type trunk
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]dis this
#
interface GigabitEthernet0/0/3
 eth-trunk 1
 lacp priority 100
#
return
[LSW1-GigabitEthernet0/0/3]q
[LSW1]int eth
[LSW1]int Eth-Trunk 1
[LSW1-Eth-Trunk1]port li
[LSW1-Eth-Trunk1]port link-type t
[LSW1-Eth-Trunk1]port link-type trunk
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW1-Eth-Trunk1]port tru
[LSW1-Eth-Trunk1]port trunk a;;
[LSW1-Eth-Trunk1]port trunk all
[LSW1-Eth-Trunk1]port trunk allow-pass vlan 10 20
Info: This operation may take a few seconds. Please wait a moment.done.
[LSW1-Eth-Trunk1]q
[LSW1]int g0/0/3
[LSW1-GigabitEthernet0/0/3]port trunk allow-pass vlan 10 20
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]port link-type trunk
                                ^
Error: Unrecognized command found at '^' position.
[LSW1-GigabitEthernet0/0/3]port li
[LSW1-GigabitEthernet0/0/3]dis this
#
interface GigabitEthernet0/0/3
 eth-trunk 1
 lacp priority 100
#
return
[LSW1-GigabitEthernet0/0/3]q
[LSW1]disp eth
[LSW1]disp eth-trunk 1
Eth-Trunk1's state information is:
Local:
LAG ID: 1                   WorkingMode: LACP
Preempt Delay: Disabled     Hash arithmetic: According to SIP-XOR-DIP
System Priority: 100        System ID: 642c-acc1-65e0
Least Active-linknumber: 1  Max Active-linknumber: 2
Operate status: up          Number Of Up Port In Trunk: 2
--------------------------------------------------------------------------------
ActorPortName          Status   PortType PortPri PortNo PortKey PortState Weight
GigabitEthernet0/0/3   Selected 1GE      100     1      305     10111100  1
GigabitEthernet0/0/4   Selected 1GE      100     2      305     10111100  1
GigabitEthernet0/0/5   Unselect 1GE      32768   3      305     10100000  1

Partner:
--------------------------------------------------------------------------------
ActorPortName          SysPri   SystemID        PortPri PortNo PortKey PortState
GigabitEthernet0/0/3   32768    6012-3c9a-61f0  32768   1      305     10111100
GigabitEthernet0/0/4   32768    6012-3c9a-61f0  32768   2      305     10111100
GigabitEthernet0/0/5   32768    6012-3c9a-61f0  32768   3      305     10110000

[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]disp th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
#
return
[LSW1-GigabitEthernet0/0/1]q
[LSW1]disp vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1]disp port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1 10 20
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW1]
[LSW1]ping 192.168.10.2
  PING 192.168.10.2: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.2 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1]ping 192.168.10
Error: Unknown host 192.168.10.
[LSW1]ping 192.168.10.1
  PING 192.168.10.1: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.1 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1]disp port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1 10 20
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW1]
[LSW1]disp vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1]int eth
[LSW1]int Eth-Trunk 1
[LSW1-Eth-Trunk1]disp this
#
interface Eth-Trunk1
 port link-type trunk
 port trunk allow-pass vlan 10 20
 mode lacp
 max active-linknumber 2
#
return
[LSW1-Eth-Trunk1]q
[LSW1]disp eth
[LSW1]disp eth-trunk 1
Eth-Trunk1's state information is:
Local:
LAG ID: 1                   WorkingMode: LACP
Preempt Delay: Disabled     Hash arithmetic: According to SIP-XOR-DIP
System Priority: 100        System ID: 642c-acc1-65e0
Least Active-linknumber: 1  Max Active-linknumber: 2
Operate status: up          Number Of Up Port In Trunk: 2
--------------------------------------------------------------------------------
ActorPortName          Status   PortType PortPri PortNo PortKey PortState Weight
GigabitEthernet0/0/3   Selected 1GE      100     1      305     10111100  1
GigabitEthernet0/0/4   Selected 1GE      100     2      305     10111100  1
GigabitEthernet0/0/5   Unselect 1GE      32768   3      305     10100000  1

Partner:
--------------------------------------------------------------------------------
ActorPortName          SysPri   SystemID        PortPri PortNo PortKey PortState
GigabitEthernet0/0/3   32768    6012-3c9a-61f0  32768   1      305     10111100
GigabitEthernet0/0/4   32768    6012-3c9a-61f0  32768   2      305     10111100
GigabitEthernet0/0/5   32768    6012-3c9a-61f0  32768   3      305     10110000

[LSW1]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Error: Authentication fail

Username:
Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 14:03:54  Failed: 1

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW1>sys
Enter system view, return user view with Ctrl+Z.
[LSW1]int eth
[LSW1]int Eth-Trunk 1
[LSW1-Eth-Trunk1]port trunk allow
[LSW1-Eth-Trunk1]port trunk allow-pass vla
[LSW1-Eth-Trunk1]port trunk allow-pass vlan all
Info: This operation may take a few seconds. Please wait a moment.done.
[LSW1-Eth-Trunk1]dis this
#
interface Eth-Trunk1
 port link-type trunk
 port trunk allow-pass vlan 2 to 4094
 mode lacp
 max active-linknumber 2
#
return
[LSW1-Eth-Trunk1]q
[LSW1]disp vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1]disp port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1-4094
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094
GigabitEthernet0/0/24       auto         1     1-4094

[LSW1]int vlanif 2
[LSW1-Vlanif2]ip addr 192.168.10.3
                                   ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif2]ip addr 192.168.10.3 24
[LSW1-Vlanif2]q
[LSW1]int vlanif 3
[LSW1-Vlanif3]ip addr 192.168.20.3
                                   ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif3]ip addr 192.168.20.3 24
[LSW1-Vlanif3]q
[LSW1]disp ip int
[LSW1]disp ip interface br
[LSW1]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 3
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 4

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           192.168.10.3/24      down       down
Vlanif3                           192.168.20.3/24      down       down

[LSW1]vlanif 3
      ^
Error: Unrecognized command found at '^' position.
[LSW1]int vlanif 3
[LSW1-Vlanif3]dis this
#
interface Vlanif3
 ip address 192.168.20.3 255.255.255.0
#
return
[LSW1-Vlanif3]start
              ^
Error: Unrecognized command found at '^' position.
[LSW1-Vlanif3]undo shutdown
Info: Interface Vlanif3 is not shutdown.
[LSW1-Vlanif3]start
              ^
Error: Unrecognized command found at '^' position.
[LSW1-Vlanif3]disp ip int
[LSW1-Vlanif3]disp ip interface bri
[LSW1-Vlanif3]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 3
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 4

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           192.168.10.3/24      down       down
Vlanif3                           192.168.20.3/24      down       down

[LSW1-Vlanif3]dis int vlanif 2
Vlanif2 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.10.3/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e3
Current system time: 2024-11-30 14:16:51
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1-Vlanif3]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1-4094
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094
GigabitEthernet0/0/24       auto         1     1-4094
GigabitEthernet0/0/25       auto         1     1-4094
GigabitEthernet0/0/26       auto         1     1-4094
GigabitEthernet0/0/27       auto         1     1-4094
GigabitEthernet0/0/28       auto         1     1-4094
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]
[LSW1-Vlanif3]disp ip int br
[LSW1-Vlanif3]disp ip int brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 3
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 4

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           192.168.10.3/24      down       down
Vlanif3                           192.168.20.3/24      down       down

[LSW1-Vlanif3]disp ip int brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 3
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 4

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           192.168.10.3/24      down       down
Vlanif3                           192.168.20.3/24      down       down

[LSW1-Vlanif3]dis vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1-Vlanif3]dis vlan 2
Error: The VLAN does not exist.
[LSW1-Vlanif3]dis vlan 20
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
20   enable  default       enable  disable    VLAN 0020
[LSW1-Vlanif3]dis vlan 10
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
10   enable  default       enable  disable    VLAN 0010
[LSW1-Vlanif3]int vlanif 2
[LSW1-Vlanif2]undo shutdown
Info: Interface Vlanif2 is not shutdown.
[LSW1-Vlanif2]dis th
#
interface Vlanif2
 ip address 192.168.10.3 255.255.255.0
#
return
[LSW1-Vlanif2]dis int vlanif 2
Vlanif2 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.10.3/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e3
Current system time: 2024-11-30 14:28:09
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1-Vlanif2]undo ip addr
[LSW1-Vlanif2]int vlanif 3
[LSW1-Vlanif3]un ip addr
[LSW1-Vlanif3]dis th
#
interface Vlanif3
#
return
[LSW1-Vlanif3]q
[LSW1]int vlanif 10
[LSW1-Vlanif10]ip addr 192.168.10.3
                                    ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif10]ip addr 192.168.10.3 24
[LSW1-Vlanif10]int vlanif 20
[LSW1-Vlanif20]ip addr 192.168.20.3 24
[LSW1-Vlanif20]q
[LSW1]ping 192.168.20.3
  PING 192.168.20.3: 56  data bytes, press CTRL_C to break
    Reply from 192.168.20.3: bytes=56 Sequence=1 ttl=255 time=1 ms
    Reply from 192.168.20.3: bytes=56 Sequence=2 ttl=255 time=2 ms
    Reply from 192.168.20.3: bytes=56 Sequence=3 ttl=255 time=1 ms
    Reply from 192.168.20.3: bytes=56 Sequence=4 ttl=255 time=5 ms
    Reply from 192.168.20.3: bytes=56 Sequence=5 ttl=255 time=2 ms

  --- 192.168.20.3 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/2/5 ms

[LSW1]ping 192.168.20.1
  PING 192.168.20.1: 56  data bytes, press CTRL_C to break
    Reply from 192.168.20.1: bytes=56 Sequence=1 ttl=128 time=1 ms
    Reply from 192.168.20.1: bytes=56 Sequence=2 ttl=128 time=1 ms
    Reply from 192.168.20.1: bytes=56 Sequence=3 ttl=128 time=1 ms
    Reply from 192.168.20.1: bytes=56 Sequence=4 ttl=128 time=1 ms
    Reply from 192.168.20.1: bytes=56 Sequence=5 ttl=128 time=1 ms

  --- 192.168.20.1 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/1/1 ms

[LSW1]ping 192.168.20.2
  PING 192.168.20.2: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.20.2 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1]ping 192.168.10.1
  PING 192.168.10.1: 56  data bytes, press CTRL_C to break
    Reply from 192.168.10.1: bytes=56 Sequence=1 ttl=128 time=1 ms
    Reply from 192.168.10.1: bytes=56 Sequence=2 ttl=128 time=1 ms
    Reply from 192.168.10.1: bytes=56 Sequence=3 ttl=128 time=1 ms
    Reply from 192.168.10.1: bytes=56 Sequence=4 ttl=128 time=1 ms
    Reply from 192.168.10.1: bytes=56 Sequence=5 ttl=128 time=1 ms

  --- 192.168.10.1 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/1/1 ms

[LSW1]dis vlanif 10
          ^
Error: Unrecognized command found at '^' position.
[LSW1]dis int vlanif 10
Vlanif10 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-11-30 14:29:36
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.10.3/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65eb
Current system time: 2024-11-30 14:31:15
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]ping 192.168.10.2
  PING 192.168.10.2: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.2 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1-4094
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW1]
[LSW1]dis vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1]disp vlanif 10
           ^
Error: Unrecognized command found at '^' position.
[LSW1]disp int vlanif 10
Vlanif10 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-11-30 14:29:36
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.10.3/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65eb
Current system time: 2024-11-30 14:44:01
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]int vlanif 10
[LSW1-Vlanif10]undo ip add
[LSW1-Vlanif10]undo ip address
[LSW1-Vlanif10]dis this
#
interface Vlanif10
#
return
[LSW1-Vlanif10]int vla
[LSW1-Vlanif10]int vlanif 20
[LSW1-Vlanif20]undo ip add
[LSW1-Vlanif20]undo ip address
[LSW1-Vlanif20]shut
[LSW1-Vlanif20]shutdown
[LSW1-Vlanif20]int vlanif 10
[LSW1-Vlanif10]shutdown
[LSW1-Vlanif10]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 14:04:05  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW1>sys
Enter system view, return user view with Ctrl+Z.
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]port-s
[LSW1-GigabitEthernet0/0/1]port-security enable
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/1]port-security mac-
[LSW1-GigabitEthernet0/0/1]port-security mac-address st
[LSW1-GigabitEthernet0/0/1]port-security mac-address sticky
[LSW1-GigabitEthernet0/0/1]port-s
[LSW1-GigabitEthernet0/0/1]port-security max
[LSW1-GigabitEthernet0/0/1]port-security max-mac-num 1
[LSW1-GigabitEthernet0/0/1]q
[LSW1]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 16:00:42  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW1>sys
Enter system view, return user view with Ctrl+Z.
[LSW1]int vlanif 10
[LSW1-Vlanif10]ip ad
[LSW1-Vlanif10]ip address 192.168.10.5
                                       ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif10]ip address 192.168.10.5 24
[LSW1-Vlanif10]int vlanif 20
[LSW1-Vlanif20]ip add 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]disp ip int br
[LSW1-Vlanif20]disp ip int brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 2
The number of interface that is DOWN in Physical is 5
The number of interface that is UP in Protocol is 1
The number of interface that is DOWN in Protocol is 6

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           unassigned           down       down
Vlanif3                           unassigned           down       down
Vlanif10                          192.168.10.5/24      *down      down
Vlanif20                          unassigned           *down      down

[LSW1-Vlanif20]ping 192.168.10.5
  PING 192.168.10.5: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.10.5 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1-Vlanif20]q
[LSW1]ping 192.168.10.5
  PING 192.168.10.5: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.5 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW1]int vl
[LSW1]int Vlanif 2
[LSW1-Vlanif2]ip addr 192.168.10.6
                                   ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif2]ip addr 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif2]dis this
#
interface Vlanif2
#
return
[LSW1-Vlanif2]int Vlanif 20
[LSW1-Vlanif20]dis this
#
interface Vlanif20
 shutdown
#
return
[LSW1-Vlanif20]ip addr 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]ip addr 192.168.20.6 24
[LSW1-Vlanif20]ip addr 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]ip addr 192.168.10.5 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]ip addr 192.168.10.8 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]ip addr 192.168.20.8 24
[LSW1-Vlanif20]ip addr 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]int v
[LSW1-Vlanif20]int vl
[LSW1-Vlanif20]int vlan
[LSW1-Vlanif20]int vlanif 10
[LSW1-Vlanif10]undo shut
[LSW1-Vlanif10]disp ip int
[LSW1-Vlanif10]disp ip interface b
[LSW1-Vlanif10]disp ip interface brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 3
The number of interface that is DOWN in Physical is 4
The number of interface that is UP in Protocol is 2
The number of interface that is DOWN in Protocol is 5

Interface                         IP Address/Mask      Physical   Protocol
MEth0/0/1                         192.168.1.253/24     down       down
NULL0                             unassigned           up         up(s)
Vlanif1                           unassigned           up         down
Vlanif2                           unassigned           down       down
Vlanif3                           unassigned           down       down
Vlanif10                          192.168.10.5/24      up         up
Vlanif20                          192.168.20.8/24      *down      down

[LSW1-Vlanif10]int vlanif 20
[LSW1-Vlanif20]undo shut
[LSW1-Vlanif20]undo shutdown
[LSW1-Vlanif20]dis this
#
interface Vlanif20
 ip address 192.168.20.8 255.255.255.0
#
return
[LSW1-Vlanif20]ip addr 192.168.10.6
                                    ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif20]ip addr 192.168.10.6 24
Error: The specified address conflicts with another address.
[LSW1-Vlanif20]ip addr 192.168.20.6 24
[LSW1-Vlanif20]disp ip vlanif all
                       ^
Error: Unrecognized command found at '^' position.
[LSW1-Vlanif20]disp vlan
[LSW1-Vlanif20]disp vlanif 20
                    ^
Error: Unrecognized command found at '^' position.
[LSW1-Vlanif20]disp int vlanif all
                               ^
Error: Wrong parameter found at '^' position.
[LSW1-Vlanif20]disp int vlanif
Vlanif1 current state : UP
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e2
Current system time: 2024-11-30 16:41:09
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

Vlanif2 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e3
Current system time: 2024-11-30 16:41:09
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

Vlanif3 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500

[LSW1-Vlanif20]dis this
#
interface Vlanif20
 ip address 192.168.20.6 255.255.255.0
#
return
[LSW1-Vlanif20]dis vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW1-Vlanif20]dis this
#
interface Vlanif20
 ip address 192.168.20.6 255.255.255.0
#
return
[LSW1-Vlanif20]dis vlanif 20
               ^
Error:Ambiguous command found at '^' position.
[LSW1-Vlanif20]q
[LSW1]dis vlanif 20
          ^
Error: Unrecognized command found at '^' position.
[LSW1]dis int vlanif 20
Vlanif20 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-11-30 16:30:54
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.20.6/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e6
Current system time: 2024-11-30 16:42:36
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]ping 192.168.20.6
  PING 192.168.20.6: 56  data bytes, press CTRL_C to break
    Reply from 192.168.20.6: bytes=56 Sequence=1 ttl=255 time=1 ms
    Reply from 192.168.20.6: bytes=56 Sequence=2 ttl=255 time=1 ms
    Reply from 192.168.20.6: bytes=56 Sequence=3 ttl=255 time=1 ms
    Reply from 192.168.20.6: bytes=56 Sequence=4 ttl=255 time=2 ms
    Reply from 192.168.20.6: bytes=56 Sequence=5 ttl=255 time=33 ms

  --- 192.168.20.6 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/7/33 ms

[LSW1]ping 192.168.20.2
  PING 192.168.20.2: 56  data bytes, press CTRL_C to break
    Reply from 192.168.20.2: bytes=56 Sequence=1 ttl=128 time=1 ms
    Reply from 192.168.20.2: bytes=56 Sequence=2 ttl=128 time=1 ms
    Reply from 192.168.20.2: bytes=56 Sequence=3 ttl=128 time=1 ms
    Reply from 192.168.20.2: bytes=56 Sequence=4 ttl=128 time=1 ms
    Reply from 192.168.20.2: bytes=56 Sequence=5 ttl=128 time=1 ms

  --- 192.168.20.2 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/1/1 ms

[LSW1]ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Reply from 192.168.10.3: bytes=56 Sequence=1 ttl=128 time=1 ms
    Reply from 192.168.10.3: bytes=56 Sequence=2 ttl=128 time=1 ms
    Reply from 192.168.10.3: bytes=56 Sequence=3 ttl=128 time=1 ms
    Reply from 192.168.10.3: bytes=56 Sequence=4 ttl=128 time=1 ms
    Reply from 192.168.10.3: bytes=56 Sequence=5 ttl=128 time=1 ms

  --- 192.168.10.3 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/1/1 ms

[LSW1]ping 192.168.20.4
  PING 192.168.20.4: 56  data bytes, press CTRL_C to break
    Reply from 192.168.20.4: bytes=56 Sequence=1 ttl=128 time=1 ms
    Reply from 192.168.20.4: bytes=56 Sequence=2 ttl=128 time=1 ms
    Reply from 192.168.20.4: bytes=56 Sequence=3 ttl=128 time=1 ms
    Reply from 192.168.20.4: bytes=56 Sequence=4 ttl=128 time=1 ms
    Reply from 192.168.20.4: bytes=56 Sequence=5 ttl=128 time=1 ms

  --- 192.168.20.4 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 1/1/1 ms

[LSW1]int vlanif 10
[LSW1-Vlanif10]ip addr 192.168.10.5
                                    ^
Error:Incomplete command found at '^' position.
[LSW1-Vlanif10]ip addr 192.168.10.5 24
[LSW1-Vlanif10]int vlanif 20
[LSW1-Vlanif20]ip addr 192.168.20.6 24
[LSW1-Vlanif20]q
[LSW1]dis vlanif all
          ^
Error: Unrecognized command found at '^' position.
[LSW1]dis ip vlanif all
             ^
Error: Unrecognized command found at '^' position.
[LSW1]dis int vlanif all
                     ^
Error: Wrong parameter found at '^' position.
[LSW1]dis int vlanif
Vlanif1 current state : UP
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e2
Current system time: 2024-11-30 16:47:36
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

Vlanif2 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e3
Current system time: 2024-11-30 16:47:36
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

Vlanif3 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500

[LSW1]dis int vlanif 10
Vlanif10 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-11-30 16:28:13
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.10.5/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65eb
Current system time: 2024-11-30 16:56:22
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]dis int vlanif 20
Vlanif20 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-11-30 16:30:54
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 192.168.20.6/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 642c-acc1-65e6
Current system time: 2024-11-30 16:56:26
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]dis int vlanif all
                     ^
Error: Wrong parameter found at '^' position.
[LSW1]dis int vlanif 10 20
                        ^
Error:Too many parameters found at '^' position.
[LSW1]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 16:21:55  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW1>sys
Enter system view, return user view with Ctrl+Z.
[LSW1]int g0/0/0
          ^
Error: Wrong parameter found at '^' position.
[LSW1]int g0/0/2
[LSW1-GigabitEthernet0/0/2]int g0/0/2
[LSW1-GigabitEthernet0/0/2]int g0/0/1
[LSW1-GigabitEthernet0/0/1]di th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]undo port-st
[LSW1-GigabitEthernet0/0/1]undo port-s
[LSW1-GigabitEthernet0/0/1]undo port-security enable
Error: Sticky MAC is not disabled.
[LSW1-GigabitEthernet0/0/1]dis th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]undo port-security
                                              ^
Error:Incomplete command found at '^' position.
[LSW1-GigabitEthernet0/0/1]undo port-s
[LSW1-GigabitEthernet0/0/1]undo port-security mac-
[LSW1-GigabitEthernet0/0/1]undo port-security mac-address s
[LSW1-GigabitEthernet0/0/1]undo port-security mac-address sticky
[LSW1-GigabitEthernet0/0/1]undo port-security enable
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/1]di th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
#
return
[LSW1-GigabitEthernet0/0/1] port-security enable
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/1]port-security mac-address sticky
[LSW1-GigabitEthernet0/0/1]port-s
[LSW1-GigabitEthernet0/0/1]port-security max-mac-
[LSW1-GigabitEthernet0/0/1]port-security max-mac-num 1
[LSW1-GigabitEthernet0/0/1]q
[LSW1]dis mac-ad
[LSW1]dis mac-address sec
[LSW1]dis mac-address security-c
[LSW1]dis mac-address security
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
Total items displayed = 0

[LSW1]dis mac-address sec-con
[LSW1]dis mac-address sec-config
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
Total items displayed = 0

[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]dis thi
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]port-security mac-address sticky vlan 10
                                                            ^
Error: Wrong parameter found at '^' position.
[LSW1-GigabitEthernet0/0/1]dip mac
[LSW1-GigabitEthernet0/0/1]q
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]disp mac
[LSW1-GigabitEthernet0/0/1]disp mac-ad
[LSW1-GigabitEthernet0/0/1]disp mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
6c24-08ca-2d8a 10/-/-                            GE0/0/1             sticky

-------------------------------------------------------------------------------
Total items displayed = 2

[LSW1-GigabitEthernet0/0/1]dis th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]mac-addre
[LSW1-GigabitEthernet0/0/1]mac-address lear
[LSW1-GigabitEthernet0/0/1]mac-address learning en
[LSW1-GigabitEthernet0/0/1]mac-address learning
                                                ^
Error:Incomplete command found at '^' position.
[LSW1-GigabitEthernet0/0/1]mac-address learning disab
[LSW1-GigabitEthernet0/0/1]mac-address learning disable
[LSW1-GigabitEthernet0/0/1]di th
#
interface GigabitEthernet0/0/1
 port link-type access
 mac-address learning disable
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]undo mac-address learning disable
[LSW1-GigabitEthernet0/0/1]disp mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
1c69-7a2e-b0dc 10/-/-                            Eth-Trunk1          dynamic
6c24-08ca-2d8a 10/-/-                            GE0/0/1             sticky
1c69-7a2f-8e46 20/-/-                            GE0/0/2             dynamic
1c69-7a2f-9f0d 20/-/-                            Eth-Trunk1          dynamic

-------------------------------------------------------------------------------
Total items displayed = 5

[LSW1-GigabitEthernet0/0/1]undo mac-ad
[LSW1-GigabitEthernet0/0/1]undo port-
[LSW1-GigabitEthernet0/0/1]undo port-s
[LSW1-GigabitEthernet0/0/1]undo port-security mac
[LSW1-GigabitEthernet0/0/1]undo port-security mac-address st
[LSW1-GigabitEthernet0/0/1]undo port-security mac-address sticky
[LSW1-GigabitEthernet0/0/1]und port-sc
[LSW1-GigabitEthernet0/0/1]und port-se
[LSW1-GigabitEthernet0/0/1]und port-security
                                             ^
Error:Incomplete command found at '^' position.
[LSW1-GigabitEthernet0/0/1]und port-security en
[LSW1-GigabitEthernet0/0/1]und port-security enable
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/1]dis th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
#
return
[LSW1-GigabitEthernet0/0/1]port-security
                                         ^
Error:Incomplete command found at '^' position.
[LSW1-GigabitEthernet0/0/1]port-security en
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/1]port-security mac-address sticky
[LSW1-GigabitEthernet0/0/1]disp mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
1c69-7a2f-8e43 10/-/-                            GE0/0/1             sticky
1c69-7a2f-8e46 20/-/-                            GE0/0/2             dynamic
1c69-7a2f-9f0d 20/-/-                            Eth-Trunk1          dynamic

-------------------------------------------------------------------------------
Total items displayed = 4

[LSW1-GigabitEthernet0/0/1]int g0/0/2
[LSW1-GigabitEthernet0/0/2]port-security en
Info: This operation may take a few seconds. Please wait a moment.
[LSW1-GigabitEthernet0/0/2]port-security mac-address sticky
[LSW1-GigabitEthernet0/0/2]q
[LSW1]disp mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
1c69-7a2e-b0dc 10/-/-                            Eth-Trunk1          dynamic
1c69-7a2f-8e43 10/-/-                            GE0/0/1             sticky
1c69-7a2f-8e46 20/-/-                            GE0/0/2             sticky
1c69-7a2f-9f0d 20/-/-                            Eth-Trunk1          dynamic

-------------------------------------------------------------------------------
Total items displayed = 5

[LSW1]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 17:09:21  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW1>disp mac-ad
<LSW1>disp mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
1c69-7a2e-b0dc 10/-/-                            Eth-Trunk1          dynamic
1c69-7a2f-8e43 10/-/-                            GE0/0/1             sticky
1c69-7a2f-8e46 20/-/-                            GE0/0/2             sticky
1c69-7a2f-9f0d 20/-/-                            Eth-Trunk1          dynamic

-------------------------------------------------------------------------------
Total items displayed = 5

<LSW1>sys
Enter system view, return user view with Ctrl+Z.
[LSW1]int g0/0/1
[LSW1-GigabitEthernet0/0/1]dis th
#
interface GigabitEthernet0/0/1
 port link-type access
 port default vlan 10
 port-security enable
 port-security mac-address sticky
#
return
[LSW1-GigabitEthernet0/0/1]dis mac-add
[LSW1-GigabitEthernet0/0/1]dis mac-address
-------------------------------------------------------------------------------
MAC Address    VLAN/VSI/BD                       Learned-From        Type
-------------------------------------------------------------------------------
6012-3c9a-61f0 1/-/-                             Eth-Trunk1          dynamic
1c69-7a2f-8e43 10/-/-                            GE0/0/1             sticky
1c69-7a2f-8e46 20/-/-                            GE0/0/2             sticky
1c69-7a2f-9f0d 20/-/-                            Eth-Trunk1          dynamic

-------------------------------------------------------------------------------
Total items displayed = 4

[LSW1-GigabitEthernet0/0/1]

User interface con0 is available

Please Press ENTER.