[LSW1]stp pathc
[LSW1]stp pathcost-standard lega
[LSW1]stp pathcost-standard legacy
[LSW1]dis stp
-------[CIST Global Info][Mode STP]-------
CIST Bridge         :0    .6012-3c9a-5ff0
Config Times        :Hello 2s MaxAge 20s FwDly 15s MaxHop 20
Active Times        :Hello 2s MaxAge 20s FwDly 15s MaxHop 20
CIST Root/ERPC      :0    .6012-3c9a-5ff0 / 0 (This bridge is the root)
CIST RegRoot/IRPC   :0    .6012-3c9a-5ff0 / 0
CIST RootPortId     :0.0
BPDU-Protection     :Disabled
CIST Root Type      :Primary root
TC or TCN received  :0
TC count per hello  :0
STP Converge Mode   :Normal
Share region-configuration :Enabled
Time since last TC  :0 days 0h:0m:0s
Number of TC        :0
----[Port1(GigabitEthernet0/0/1)][DOWN]----
 Port Protocol       :Enabled
 Port Role           :Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Designated Bridge/Port   :0.6012-3c9a-5ff0 / 128.1
 Port Edged          :Config=default / Active=disabled
 Point-to-point      :Config=auto / Active=false
 Transit Limit       :6 packets/s
 Protection Type     :None
 Port STP Mode       :MSTP
 Port Protocol Type  :Config=auto / Active=dot1s
 BPDU Encapsulation  :Config=stp / Active=stp
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s RemHop 20
 TC or TCN send      :0
 TC or TCN received  :0
 BPDU Sent           :0
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0
          TCN: 0, Config: 0, RST: 0, MST: 0
----[Port2(GigabitEthernet0/0/2)][DOWN]----
 Port Protocol       :Enabled
 Port Role           :Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Designated Bridge/Port   :0.6012-3c9a-5ff0 / 128.2
 Port Edged          :Config=default / Active=disabled
 Point-to-point      :Config=auto / Active=false
 Transit Limit       :6 packets/s
 Protection Type     :None
 Port STP Mode       :MSTP
 Port Protocol Type  :Config=auto / Active=dot1s
 BPDU Encapsulation  :Config=stp / Active=stp
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s RemHop 20
 TC or TCN send      :0
 TC or TCN received  :0
 BPDU Sent           :0
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0
          TCN: 0, Config: 0, RST: 0, MST: 0
----[Port3(GigabitEthernet0/0/3)][DOWN]----

[LSW1]stp enable
[LSW1]disp stp br
[LSW1]disp stp bri
 MSTID   Port                        Role  STP State     Protection
[LSW1]

Hi-Boot 2012.10 (2019-11-17 - 18:42:56)

FirBoot
Boot from bootb

Hi-Boot 2012.10 (2020-05-05 - 09:30:31)

SecBoot

Hit <ctrl+t> to stop autoboot:  0
Boot from ospkga
Starting kernel
The bootargs of l2_cache= is not on, maybe the soc haven't l2 cache
**** Total Boot time: 5133 ms, uncompress initrd cost 4631 ms ****
starting pid 952, tty '': '/etc/rc.d/rc.sysinit'
mount file system
Loading the kernel modules:
Making device instances:
Setting hostname:
Cleaning up tmp :
Setting up the sysctl configurations:
Setting up interface lo:
System booting cost:5.71 16.99
starting pid 1003, tty '/dev/ttyS0': '/etc/rc.d/rc.lsw'
Bootloader CMS check result is true
Boot from main bootloader
/

May  5 2020, 09:33:18

Last reset type: PowerOn

No need to backup uboot
Press Ctrl+B or Ctrl+E to enter BootLoad menu: 0

Startup information : 1

Read boot file: flash:/s5735s-s-v200r019c10spc500.cc

Current startup file: flash:/s5735s-s-v200r019c10spc500.cc

Info: Checking signature, please wait.......
System total memory is 0x1f200000

Start to initialize the LSW ...
Watchdog Monitor off

Watchdog Monitor on

Initializing the LSW ...................................................... done
Initializing netlink ...................................................... done
Initializing fast netlink ................................................. done
Stack status : enable
ECM Stack status : run

Initializing FSP task begin ...

Initializing DEV module ................................................... done

Initializing hardware system .............................................. done
Begin to start the system ...

Registering IPC and VP callback to platform ............................... done

Initializing VFS ..................................... Done
Checking startup system-software .......................................... done
Reading PAF file .......................................................... done
Initializing VOS monitor ............................. Done
CFM initialization advance ........................... done
Initializing PAT ..................................... Done
Initializing HA ...................................... done
VFS registering to HA ................................ Done

VRP root begin ...
VRP root end
CFG initialization begin ............................. done
CFM initialization begin ............................. done
CLI initialization begin ............................. done
Registering VRP all link command begin ............... Done
Creating task begin ...
Creating task end
Task initialization begin ...
Task initialization end

ECMM status : run
Cmd registering begin ...
Cmd registering end

Task awake begin ...
Task awake end

Recover configuration begin ...
Recover configuration end
Press ENTER to get started.

Login authentication

Username:admin
Password:
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW2>disp stp int g0/0/1 br
 MSTID   Port                        Role  STP State     Protection
    0    GigabitEthernet0/0/1        DESI  FORWARDING      NONE
<LSW2>

Login authentication

Username:admin
Password:
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW3>disp stp int g0/0/1 br
 MSTID   Port                        Role  STP State     Protection
    0    GigabitEthernet0/0/1        ALTE  DISCARDING      NONE
<LSW3>disp stp br
 MSTID   Port                        Role  STP State     Protection
    0    GigabitEthernet0/0/1        ALTE  DISCARDING      NONE
    0    GigabitEthernet0/0/2        DESI  FORWARDING      BPDU
    0    GigabitEthernet0/0/3        ROOT  FORWARDING      NONE
<LSW3>
[LSW1]
[LSW1]disp stp bri
 MSTID   Port                        Role  STP State     Protection
    0    GigabitEthernet0/0/1        DESI  FORWARDING      NONE
    0    GigabitEthernet0/0/2        DESI  FORWARDING      NONE
[LSW1]

Login authentication

Username:admin
Password:
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW4>dis stp br
 MSTID   Port                        Role  STP State     Protection
    0    GigabitEthernet0/0/1        ROOT  FORWARDING      NONE
    0    GigabitEthernet0/0/2        DESI  FORWARDING      NONE
<LSW4>