*** C1350T01 start *******************************
parent is waiting SIGUSR1
child is sending SIGUSR1 (should be caught)
suspender caught SIGUSR1
sigsuspend return -1 as expected
[OK] caught SIGUSR1
*** C1350T01 PASSED ******************************

*** C1350T02 start *******************************
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
rt_sigsuspend01.c:53: PASS: rt_sigsuspend() returned with -1 and EINTR
rt_sigsuspend01.c:62: PASS: signal mask preserved

Summary:
passed   2
failed   0
skipped  0
warnings 0
*** C1350T02 PASSED (0)

*** C1350T03 start *******************************
sigsuspend01    1  TPASS  :  Functionality of sigsuspend() successful
*** C1350T03 PASSED (1)

*** C1350T04 start *******************************
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
pause01.c:35: PASS: pause() interrupted with EINTR

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1350T04 PASSED (0)

*** C1350T05 start *******************************
pause02     1  TPASS  :  pause was interrupted correctly
*** C1350T05 PASSED (1)

*** C1350T06 start *******************************
pause03     1  TPASS  :  pause() did not return after SIGKILL
*** C1350T06 PASSED (1)

