*** C1350T01 start *******************************
parent is waiting SIGUSR1
child is sending SIGUSR1 (should be caught)
suspender caught SIGUSR1
sigsuspend return -1 as expected
[OK] caught SIGUSR1
*** C1350T01 PASSED ******************************

*** C1350T02 start *******************************
rt_sigsuspend01    1  TPASS  :  rt_sigsuspend PASSED
*** C1350T02 PASSED (1)

*** C1350T03 start *******************************
sigsuspend01    1  TPASS  :  Functionality of sigsuspend() successful
*** C1350T03 PASSED (1)

*** C1350T04 start *******************************
pause01     1  TPASS  :  pause() returned -1
*** C1350T04 PASSED (1)

*** C1350T05 start *******************************
pause02     1  TPASS  :  pause was interrupted correctly
*** C1350T05 PASSED (1)

*** C1350T06 start *******************************
pause03     1  TPASS  :  pause() did not return after SIGKILL
*** C1350T06 PASSED (1)

