CONFIGS=-DNUM_CLUSTERS=1 -DNUM_CORES=2 -DNUM_WARPS=4 -DNUM_THREADS=4 -DL2_ENABLE=0 -DL3_ENABLE=0 -DPERF_ENABLE
make: Entering directory '/nethome/lcooper43/vortex-dev-old/driver/opae'
rm -rf libvortex.so *.o .depend
make: Leaving directory '/nethome/lcooper43/vortex-dev-old/driver/opae'
make: Entering directory '/nethome/lcooper43/vortex-dev-old/benchmarks/opencl/vecadd'
LD_LIBRARY_PATH=/opt/pocl/runtime/lib:/nethome/lcooper43/vortex-dev-old/driver/opae:/opt/opae/1.1.2/lib:/opt/inteldevstack/a10_gx_pac_ias_1_2_1_pv/opencl/opencl_bsp/linux64/lib:/opt/intelFPGA_pro/quartus_19.2.0b57/hld/host/linux64/lib:/opt/intelFPGA_pro/quartus_19.2.0b57/hld/linux64/lib: ./vecadd -n64
[VXDRV] DEVCAPS: version=0, num_cores=2, num_warps=4, num_threads=4
Create context
Allocate device buffers
Create program from kernel source
Upload source buffers
Execute the kernel
Elapsed time: 4 ms
Download destination buffer
Verify result
PASSED!
PERF: core0: instrs=2981, cycles=5416, IPC=0.550406
PERF: core0: ibuffer stalls=0
PERF: core0: scoreboard stalls=0
PERF: core0: alu unit stalls=0
PERF: core0: lsu unit stalls=0
PERF: core0: csr unit stalls=0
PERF: core0: fpu unit stalls=0
PERF: core0: gpu unit stalls=0
PERF: core0: icache reads=0
PERF: core0: icache read misses=0 (hit ratio=-2147483648%)
PERF: core0: icache pipeline stalls=0
PERF: core0: icache reponse stalls=0
PERF: core0: dcache reads=0
PERF: core0: dcache writes=0
PERF: core0: dcache read misses=0 (hit ratio=-2147483648%)
PERF: core0: dcache write misses=0 (hit ratio=-2147483648%)
PERF: core0: dcache bank stalls=0 (utilization=-2147483648%)
PERF: core0: dcache mshr stalls=0
PERF: core0: dcache pipeline stalls=0
PERF: core0: dcache reponse stalls=0
PERF: core0: smem reads=0
PERF: core0: smem writes=0
PERF: core0: smem bank stalls=0 (utilization=-2147483648%)
PERF: core0: dram requests=0 (reads=0, writes=0)
PERF: core0: dram stalls=0 (utilization=-2147483648%)
PERF: core0: dram average latency=-2147483648 cycles
PERF: core1: instrs=2983, cycles=5353, IPC=0.557258
PERF: core1: ibuffer stalls=0
PERF: core1: scoreboard stalls=0
PERF: core1: alu unit stalls=0
PERF: core1: lsu unit stalls=0
PERF: core1: csr unit stalls=0
PERF: core1: fpu unit stalls=0
PERF: core1: gpu unit stalls=0
PERF: core1: icache reads=0
PERF: core1: icache read misses=0 (hit ratio=-2147483648%)
PERF: core1: icache pipeline stalls=0
PERF: core1: icache reponse stalls=0
PERF: core1: dcache reads=0
PERF: core1: dcache writes=0
PERF: core1: dcache read misses=0 (hit ratio=-2147483648%)
PERF: core1: dcache write misses=0 (hit ratio=-2147483648%)
PERF: core1: dcache bank stalls=0 (utilization=-2147483648%)
PERF: core1: dcache mshr stalls=0
PERF: core1: dcache pipeline stalls=0
PERF: core1: dcache reponse stalls=0
PERF: core1: smem reads=0
PERF: core1: smem writes=0
PERF: core1: smem bank stalls=0 (utilization=-2147483648%)
PERF: core1: dram requests=0 (reads=0, writes=0)
PERF: core1: dram stalls=0 (utilization=-2147483648%)
PERF: core1: dram average latency=-2147483648 cycles
PERF: instrs=5964, cycles=5416, IPC=1.101182
PERF: ibuffer stalls=0
PERF: scoreboard stalls=0
PERF: alu unit stalls=0
PERF: lsu unit stalls=0
PERF: csr unit stalls=0
PERF: fpu unit stalls=0
PERF: gpu unit stalls=0
PERF: icache reads=0
PERF: icache read misses=0 (hit ratio=-2147483648%)
PERF: icache pipeline stalls=0
PERF: icache reponse stalls=0
PERF: dcache reads=0
PERF: dcache writes=0
PERF: dcache read misses=0 (hit ratio=-2147483648%)
PERF: dcache write misses=0 (hit ratio=-2147483648%)
PERF: dcache bank stalls=0 (utilization=-2147483648%)
PERF: dcache mshr stalls=0
PERF: dcache pipeline stalls=0
PERF: dcache reponse stalls=0
PERF: smem reads=0
PERF: smem writes=0
PERF: smem bank stalls=0 (utilization=-2147483648%)
PERF: dram requests=0 (reads=0, writes=0)
PERF: dram stalls=0 (utilization=-2147483648%)
PERF: dram average latency=-2147483648 cycles
make: Leaving directory '/nethome/lcooper43/vortex-dev-old/benchmarks/opencl/vecadd'
