# vsim rf2_32x128_wm1_tb -c -lib rf_lib -do "vcd file rf2_32x128_wm1_tb.vcd; vcd add -r /rf2_32x128_wm1_tb/*; run -all; quit -f" 
# Start time: 13:02:14 on Oct 29,2019
# ** Note: (vsim-3813) Design is being optimized due to module recompilation...
# //  ModelSim SE-64 10.6a Mar 16 2017Linux 3.10.0-1062.1.2.el7.x86_64
# //
# //  Copyright 1991-2017 Mentor Graphics Corporation
# //  All Rights Reserved.
# //
# //  ModelSim SE-64 and its associated documentation contain trade
# //  secrets and commercial or financial information that are the property of
# //  Mentor Graphics Corporation and are privileged, confidential,
# //  and exempt from disclosure under the Freedom of Information Act,
# //  5 U.S.C. Section 552. Furthermore, this information
# //  is prohibited from disclosure under the Trade Secrets Act,
# //  18 U.S.C. Section 1905.
# //
# Loading sv_std.std
# Loading work.rf2_32x128_wm1_tb(fast)
# Loading work.rf2_32x128_wm1(fast)
# vcd file rf2_32x128_wm1_tb.vcd
#  vcd add -r /rf2_32x128_wm1_tb/*
#  run -all
# ** Note: $finish    : rf2_32x128_wm1_tb.v(42)
#    Time: 220 ns  Iteration: 0  Instance: /rf2_32x128_wm1_tb
# End time: 13:02:16 on Oct 29,2019, Elapsed time: 0:00:02
# Errors: 0, Warnings: 0
