*** C1291T01 start *******************************
mmap13      1  TPASS  :  Got SIGBUS as expected
*** C1291T01 PASSED (1)

*** C1291T02 start *******************************
/dev/mem is not exist
*** C1291T02 SKIP

*** C1291T03 start *******************************
** FileMap(2pages) /dev/zero and read
value: 0x0
Touch head of 1st page: OK
value: 0x0
Touch middle of 1st page: OK
value: 0x0
Touch middle of 2nd page: OK
*** C1291T03 PASSED

*** C1291T04 start *******************************
sh: line 1: 26262 Segmentation fault      grep XYZ /tmp/mmaADcyci/mmapfile > /dev/null
mmap01      1  TPASS  :  Functionality of mmap() successful
*** C1291T04 PASSED (1)

*** C1291T05 start *******************************
mmap02      1  TPASS  :  Functionality of mmap() successful
*** C1291T05 PASSED (1)

*** C1291T06 start *******************************
mmap03      1  TPASS  :  mmap() functionality is correct
*** C1291T06 PASSED (1)

*** C1291T07 start *******************************
mmap04      1  TPASS  :  Functionality of mmap() successful
*** C1291T07 PASSED (1)

*** C1291T08 start *******************************
mmap05      1  TPASS  :  Got SIGSEGV as expected
*** C1291T08 PASSED (1)

*** C1291T09 start *******************************
mmap06      1  TPASS  :  mmap failed with EACCES
*** C1291T09 PASSED (1)

*** C1291T10 start *******************************
mmap07      1  TPASS  :  mmap failed with EACCES
*** C1291T10 PASSED (1)

*** C1291T11 start *******************************
mmap08      1  TPASS  :  mmap failed with EBADF
*** C1291T11 PASSED (1)

*** C1291T12 start *******************************
mmap09      1  TPASS  :  ftruncate mmaped file to a smaller size
mmap09      2  TPASS  :  ftruncate mmaped file to a larger size
mmap09      3  TPASS  :  ftruncate mmaped file to 0 size
*** C1291T12 PASSED (3)

*** C1291T13 start *******************************
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
mmap12.c:103: INFO: All pages are present
mmap12.c:127: PASS: File mapped properly

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1291T13 PASSED (0)

*** C1291T14 start *******************************
mmap14      1  TPASS  :  Functionality of mmap() successful
*** C1291T14 PASSED (1)

*** C1291T15 start *******************************
mmap15      1  TPASS  :  mmap into high region failed as expected: errno=ENOMEM(12): Cannot allocate memory
*** C1291T15 PASSED (1)

